NORMAL COUNT

PSAU

Threshold : 250mV

Gain: 25

V\_b : 54mv

LED

4

Con trigger del led non della PSAU

DIGITIZER

Gate 200

Pre Gate 72

DARK COUNT

PSAU

Vb: 54mV

Th: -6mV

DIGITIZER

Gain: 25

Gate: 100

Pre-Gate:200